(kicad_pcb (version 20221018) (generator pcbnew)

  (general
    (thickness 1.6)
  )

  (paper "A4")
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )

  (setup
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions false)
      (usegerberattributes true)
      (usegerberadvancedattributes true)
      (creategerberjobfile true)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "")
    )
  )

  (net 0 "")
  (net 1 "Net-(J1-Pin_2)")
  (net 2 "GND")
  (net 3 "Net-(J1-Pin_3)")
  (net 4 "Net-(Q3-G)")
  (net 5 "Net-(J1-Pin_4)")
  (net 6 "Net-(BT1-+)")
  (net 7 "unconnected-(U2-XTAL1{slash}PB3-Pad2)")
  (net 8 "Net-(J2-Pin_1)")
  (net 9 "Net-(J2-Pin_3)")
  (net 10 "Net-(J2-Pin_4)")
  (net 11 "Net-(J2-Pin_5)")
  (net 12 "Net-(J2-Pin_6)")

  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (tstamp 22db4a31-6da7-4c0c-8b76-28c75d0c66d6)
    (at 86.36 91.44 90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Sheetfile" "led-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "30A Id, 50V Vds, N-Channel Power MOSFET, TO-220")
    (property "ki_keywords" "N-Channel Power MOSFET")
    (path "/b5f3fa48-69ca-4b7b-8318-5560f5faba53")
    (attr through_hole)
    (fp_text reference "Q2" (at 2.54 -4.27 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2f5d5f45-22c3-4f1f-96e8-cd287c431364)
    )
    (fp_text value "BUZ11" (at 2.54 2.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 98264b3a-f475-4d49-9b07-590d21afcf41)
    )
    (fp_text user "${REFERENCE}" (at 2.54 -4.27 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 2de57f6e-3d10-4041-8637-91627d933ac7)
    )
    (fp_line (start -2.58 -3.27) (end -2.58 1.371)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ea288dc3-7e2d-4d21-b598-016824b5ae2b))
    (fp_line (start -2.58 -3.27) (end 7.66 -3.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 66c4cce4-b58a-4a35-b178-9e154df9478a))
    (fp_line (start -2.58 -1.76) (end 7.66 -1.76)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bb0ee3de-5381-45c4-9740-417a9f018217))
    (fp_line (start -2.58 1.371) (end 7.66 1.371)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0c544ce3-26e8-4f4c-935a-c6c345560639))
    (fp_line (start 0.69 -3.27) (end 0.69 -1.76)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e41f6eb6-ea8f-46dd-b85a-ec56150c2a22))
    (fp_line (start 4.391 -3.27) (end 4.391 -1.76)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6e3c008a-e131-4391-ac63-41df7e0618ec))
    (fp_line (start 7.66 -3.27) (end 7.66 1.371)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8d7c1179-1b63-416f-94ca-b70d2d1e941b))
    (fp_line (start -2.71 -3.4) (end -2.71 1.51)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e771f16e-8e51-4020-8a2b-8a3d6e6ac436))
    (fp_line (start -2.71 1.51) (end 7.79 1.51)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0d725f30-d0ab-434b-b497-4f8bf27d470a))
    (fp_line (start 7.79 -3.4) (end -2.71 -3.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4013e78a-eab2-4de7-9a18-754cb7c5ccf0))
    (fp_line (start 7.79 1.51) (end 7.79 -3.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2e5ae917-b70f-4604-99ac-8a221194f3ea))
    (fp_line (start -2.46 -3.15) (end -2.46 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c7513afc-b85b-4344-ae72-38c73b2aed4f))
    (fp_line (start -2.46 -1.88) (end 7.54 -1.88)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0b193e60-cf7f-40ae-8dd7-119881c084fe))
    (fp_line (start -2.46 1.25) (end 7.54 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 41506608-787c-4012-95b7-980a3db24e5d))
    (fp_line (start 0.69 -3.15) (end 0.69 -1.88)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp efb1f359-0b8a-49ae-9ea0-49e7bf216da3))
    (fp_line (start 4.39 -3.15) (end 4.39 -1.88)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9aa745f4-ba2b-4a4c-8cb6-66a834cf7468))
    (fp_line (start 7.54 -3.15) (end -2.46 -3.15)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a500bc26-b3b4-4290-80ba-047d577ff9a8))
    (fp_line (start 7.54 1.25) (end 7.54 -3.15)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8b7ae664-268a-4fb7-b52c-a6845d5cc098))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J2-Pin_4)") (pinfunction "G") (pintype "input") (tstamp 70bfc9fa-991e-4280-a54c-91667ba74612))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(J1-Pin_3)") (pinfunction "D") (pintype "passive") (tstamp 38abba57-cd52-4814-b0b4-cc8afb074d0c))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "S") (pintype "passive") (tstamp d368d5d5-13a3-48e4-92ab-cdff4a2e55af))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Capacitor_THT:CP_Radial_D5.0mm_P2.00mm" (layer "F.Cu")
    (tstamp 24e5a32f-21e6-4a05-81d7-802e27ca308e)
    (at 97.79 113.76 90)
    (descr "CP, Radial series, Radial, pin pitch=2.00mm, , diameter=5mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 2.00mm  diameter 5mm Electrolytic Capacitor")
    (property "Sheetfile" "led-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (path "/7d95ce59-bf2f-4a34-b557-2b74dcc46f7f")
    (attr through_hole)
    (fp_text reference "C1" (at 1 -3.75 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp b7313153-00ef-49d9-9e94-17ca62e91753)
    )
    (fp_text value "100nF" (at 1 3.75 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f74437b6-a0c7-435f-8fd7-05d0dfe0601a)
    )
    (fp_text user "${REFERENCE}" (at 1 0 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 94bfdf0f-d240-4139-b50a-b9a6d6c0394b)
    )
    (fp_line (start -1.804775 -1.475) (end -1.304775 -1.475)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 80be06c8-8930-442c-b422-f34d19daf8a7))
    (fp_line (start -1.554775 -1.725) (end -1.554775 -1.225)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f30ec4b1-7594-4bba-a2c1-fb55842fa33c))
    (fp_line (start 1 -2.58) (end 1 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d3491b06-512a-48a0-8c07-2e983225a79c))
    (fp_line (start 1 1.04) (end 1 2.58)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 47426242-51e0-4d1a-aa09-aacbeab3c426))
    (fp_line (start 1.04 -2.58) (end 1.04 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e517255b-d7d7-4330-9866-3ef6f232e228))
    (fp_line (start 1.04 1.04) (end 1.04 2.58)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 66834141-c3a7-4e6b-a26e-f014a29d4b2b))
    (fp_line (start 1.08 -2.579) (end 1.08 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 50e5e06a-acf4-4b16-8ae7-a5cd4c9c4d32))
    (fp_line (start 1.08 1.04) (end 1.08 2.579)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4366c510-5315-4e49-b656-d94f1658d8d8))
    (fp_line (start 1.12 -2.578) (end 1.12 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dc14871d-54df-4467-ad42-b036625be885))
    (fp_line (start 1.12 1.04) (end 1.12 2.578)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ea3da1a0-b9c3-4c23-9b38-b76c16ff2089))
    (fp_line (start 1.16 -2.576) (end 1.16 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c4eb82bc-9229-465c-b827-96257abf7059))
    (fp_line (start 1.16 1.04) (end 1.16 2.576)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f715b309-2634-409d-8eef-4ae090926e0c))
    (fp_line (start 1.2 -2.573) (end 1.2 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 008d874b-273d-4017-ba7e-8ed3d768505e))
    (fp_line (start 1.2 1.04) (end 1.2 2.573)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e2a8c90b-a3de-43c5-a62c-71f0aff80413))
    (fp_line (start 1.24 -2.569) (end 1.24 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp adf336e9-1459-43c2-9500-798afa528cd2))
    (fp_line (start 1.24 1.04) (end 1.24 2.569)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9241b629-cda3-4444-80ab-3b4bff7b6a17))
    (fp_line (start 1.28 -2.565) (end 1.28 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 546cb8c5-fbf2-418a-9d41-5e5f46437570))
    (fp_line (start 1.28 1.04) (end 1.28 2.565)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp da7dd396-4df2-44f8-89eb-641e82467d6b))
    (fp_line (start 1.32 -2.561) (end 1.32 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e8cea380-ffbc-44ac-a194-ad3002c368f0))
    (fp_line (start 1.32 1.04) (end 1.32 2.561)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 72d5f5b2-ca29-438a-83fa-a3835f4165e4))
    (fp_line (start 1.36 -2.556) (end 1.36 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9ed279bf-c711-4158-add5-eedab2815ae0))
    (fp_line (start 1.36 1.04) (end 1.36 2.556)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f302143a-7922-4e35-86a2-b47ab0ecde3a))
    (fp_line (start 1.4 -2.55) (end 1.4 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d8c5da78-938f-4c10-a479-dff59f1eae00))
    (fp_line (start 1.4 1.04) (end 1.4 2.55)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e5e01b6a-68ea-4934-a066-a17cd75c39e3))
    (fp_line (start 1.44 -2.543) (end 1.44 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9cb0a480-f3bd-44bf-a872-c88b10b0bff1))
    (fp_line (start 1.44 1.04) (end 1.44 2.543)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8ac3d2fd-84f9-4942-beee-1252007851d1))
    (fp_line (start 1.48 -2.536) (end 1.48 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ff4fc111-71ee-4665-ae09-f499820c32f1))
    (fp_line (start 1.48 1.04) (end 1.48 2.536)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 028a7825-c952-41b7-af94-6c8a6a97bce7))
    (fp_line (start 1.52 -2.528) (end 1.52 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4ff1960c-4bb4-4a33-ba2e-ad58f7491a00))
    (fp_line (start 1.52 1.04) (end 1.52 2.528)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 506f8f75-8ec6-4c6b-bea6-3572eb4fc60e))
    (fp_line (start 1.56 -2.52) (end 1.56 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 449f8fa0-fdab-4031-b407-7db6353476a9))
    (fp_line (start 1.56 1.04) (end 1.56 2.52)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 40f44b82-c538-4510-987f-4689439e0260))
    (fp_line (start 1.6 -2.511) (end 1.6 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0c58a059-72a9-4c58-b202-dc72f7e3dedb))
    (fp_line (start 1.6 1.04) (end 1.6 2.511)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4c90da6c-b7bd-4e86-90ca-342b1f26a720))
    (fp_line (start 1.64 -2.501) (end 1.64 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 323572a9-4d5d-4637-af84-6343f4066bea))
    (fp_line (start 1.64 1.04) (end 1.64 2.501)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3b782638-5d7e-4cd6-97c6-a3add5cd077b))
    (fp_line (start 1.68 -2.491) (end 1.68 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f23f6711-5480-4485-ac64-f762e56f94f9))
    (fp_line (start 1.68 1.04) (end 1.68 2.491)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b0065510-0078-4a2c-abd7-b3ed7591edc6))
    (fp_line (start 1.721 -2.48) (end 1.721 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 187f69dd-f08d-432e-89f8-5ac9508b3543))
    (fp_line (start 1.721 1.04) (end 1.721 2.48)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5c9b3b5e-e81b-4166-9ad6-18453d699814))
    (fp_line (start 1.761 -2.468) (end 1.761 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 73a89941-d8ed-4e82-8061-1f851703a432))
    (fp_line (start 1.761 1.04) (end 1.761 2.468)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e3a29d13-5a5d-4687-8e10-c586de1472bb))
    (fp_line (start 1.801 -2.455) (end 1.801 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0084ce6a-f041-44e6-bfd6-91ad533357e7))
    (fp_line (start 1.801 1.04) (end 1.801 2.455)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ac2a9684-7dd3-4a08-b5f0-d22567e69856))
    (fp_line (start 1.841 -2.442) (end 1.841 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 07a0d46c-36bd-48f6-b390-f389105ffed5))
    (fp_line (start 1.841 1.04) (end 1.841 2.442)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 15a09e37-53e1-474f-9ba7-3a66a7c3ad95))
    (fp_line (start 1.881 -2.428) (end 1.881 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 09bd29a6-ab02-41a7-b981-483056d68563))
    (fp_line (start 1.881 1.04) (end 1.881 2.428)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5baaa8a4-9140-4203-9cf9-db16942b0c37))
    (fp_line (start 1.921 -2.414) (end 1.921 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c779a177-f708-44d1-9569-4e9b188558c7))
    (fp_line (start 1.921 1.04) (end 1.921 2.414)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7b2202cc-4d37-41a2-93b4-4040c550cc61))
    (fp_line (start 1.961 -2.398) (end 1.961 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 99a7dad5-bb50-4891-abd4-bf2667dfdd0d))
    (fp_line (start 1.961 1.04) (end 1.961 2.398)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e2d0b886-e153-4727-9044-90d78062f78c))
    (fp_line (start 2.001 -2.382) (end 2.001 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 25b38d64-df50-4e7e-82f5-20341122b250))
    (fp_line (start 2.001 1.04) (end 2.001 2.382)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ba12f08c-0cce-451c-a747-e0819ec69d5c))
    (fp_line (start 2.041 -2.365) (end 2.041 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d4508402-fc35-4b89-8e76-024437c1dc11))
    (fp_line (start 2.041 1.04) (end 2.041 2.365)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5e377169-b850-45b9-907b-c4d6af70f8c3))
    (fp_line (start 2.081 -2.348) (end 2.081 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c8e0088f-13ec-4729-ba4e-8972d57dae73))
    (fp_line (start 2.081 1.04) (end 2.081 2.348)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e9578d54-cac0-4402-9289-99a3c18068a6))
    (fp_line (start 2.121 -2.329) (end 2.121 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0cf7c30d-4bb6-4abb-b9b4-24887ae11687))
    (fp_line (start 2.121 1.04) (end 2.121 2.329)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8168fa50-b35b-49a6-b565-3970072c5730))
    (fp_line (start 2.161 -2.31) (end 2.161 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6b96cb84-e7a5-49cf-8dd0-c0ab9de94da3))
    (fp_line (start 2.161 1.04) (end 2.161 2.31)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c632c28f-28d3-49e7-b4b6-b2a97e8c77ff))
    (fp_line (start 2.201 -2.29) (end 2.201 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d75f58f8-460c-47a8-b18e-ccd913cbf14e))
    (fp_line (start 2.201 1.04) (end 2.201 2.29)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e68af796-b0a6-4b1a-bd6b-0176f044096f))
    (fp_line (start 2.241 -2.268) (end 2.241 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9a89376d-5344-4643-980c-f753b657e194))
    (fp_line (start 2.241 1.04) (end 2.241 2.268)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b532e8d4-e341-4b08-9e03-f33a67eed6ec))
    (fp_line (start 2.281 -2.247) (end 2.281 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 281b5b99-5d5c-4c01-8ba6-d8bd1850ca08))
    (fp_line (start 2.281 1.04) (end 2.281 2.247)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c04270b8-f42b-4d73-9250-5986898c4969))
    (fp_line (start 2.321 -2.224) (end 2.321 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 400ebd97-77ad-4a58-819a-605878e15f6c))
    (fp_line (start 2.321 1.04) (end 2.321 2.224)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 45674b93-2093-4726-8505-13bac5b71993))
    (fp_line (start 2.361 -2.2) (end 2.361 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3cb9ca05-e63e-43b6-a08d-6005d052afde))
    (fp_line (start 2.361 1.04) (end 2.361 2.2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp c230ec50-03d2-496f-9278-93951c15a480))
    (fp_line (start 2.401 -2.175) (end 2.401 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ef22b5a4-be54-428b-9883-fccfa02b0373))
    (fp_line (start 2.401 1.04) (end 2.401 2.175)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3239c564-0567-4b20-af3e-9300849e23b7))
    (fp_line (start 2.441 -2.149) (end 2.441 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1f8b2fcf-309a-4dc4-bd38-d4a7598b2455))
    (fp_line (start 2.441 1.04) (end 2.441 2.149)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d2532258-1299-4dbe-93b7-4f90850eef24))
    (fp_line (start 2.481 -2.122) (end 2.481 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7efb57f1-db73-4c55-94fc-0787d3393e40))
    (fp_line (start 2.481 1.04) (end 2.481 2.122)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e59afef1-7ed8-4ff7-9d28-9033bd62c9a5))
    (fp_line (start 2.521 -2.095) (end 2.521 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cdb69d78-1587-4324-80ae-182aa748b2e3))
    (fp_line (start 2.521 1.04) (end 2.521 2.095)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5c3d0e22-231c-42b0-93c5-cb380fe9ccf4))
    (fp_line (start 2.561 -2.065) (end 2.561 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp eb153a12-1fab-4d00-8e50-40d6a2e44fa9))
    (fp_line (start 2.561 1.04) (end 2.561 2.065)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp abf6e0c7-9210-478f-a403-05823b3af8e4))
    (fp_line (start 2.601 -2.035) (end 2.601 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a3cd8cd2-8daa-4701-b807-e803f6afbe1f))
    (fp_line (start 2.601 1.04) (end 2.601 2.035)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0f4f3b06-a409-4f0b-99e5-e8eda1ee3b46))
    (fp_line (start 2.641 -2.004) (end 2.641 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cdc80964-046c-45ff-b2b0-8eef9a3034cc))
    (fp_line (start 2.641 1.04) (end 2.641 2.004)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp af9727d6-942f-4544-8b36-390cd2ab52f9))
    (fp_line (start 2.681 -1.971) (end 2.681 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ff287a41-c6c5-4e9b-a891-6fb3628e3f73))
    (fp_line (start 2.681 1.04) (end 2.681 1.971)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e0b74608-447b-47fc-9ce4-4d5ee504c5ca))
    (fp_line (start 2.721 -1.937) (end 2.721 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2efd99b4-49ab-46f6-aca3-80d3ae684b49))
    (fp_line (start 2.721 1.04) (end 2.721 1.937)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1ca44b92-16e0-4e20-a0b4-ad15b6ac9db2))
    (fp_line (start 2.761 -1.901) (end 2.761 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ef92bf29-ade3-44da-af13-b35a702664d2))
    (fp_line (start 2.761 1.04) (end 2.761 1.901)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 341ffc43-b0d9-4f06-b119-d08a33807afa))
    (fp_line (start 2.801 -1.864) (end 2.801 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0425fe27-3a5a-484f-8e89-3b29f5c0b252))
    (fp_line (start 2.801 1.04) (end 2.801 1.864)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d35f4c36-c4c9-4805-8711-793943c96017))
    (fp_line (start 2.841 -1.826) (end 2.841 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 68283d29-bee9-41c1-9726-d64116b152e2))
    (fp_line (start 2.841 1.04) (end 2.841 1.826)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e604e3d2-7524-4120-afb6-c5ba24ede1d0))
    (fp_line (start 2.881 -1.785) (end 2.881 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bb2958d7-b3a8-487c-9fe3-9356c393d088))
    (fp_line (start 2.881 1.04) (end 2.881 1.785)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 42909113-9a61-4f6f-aac9-60c1d8be5c40))
    (fp_line (start 2.921 -1.743) (end 2.921 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7a3422f5-2619-4e48-b9e7-1863cfd39e86))
    (fp_line (start 2.921 1.04) (end 2.921 1.743)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 12ba1fea-5e54-45bf-b5a9-35290a664022))
    (fp_line (start 2.961 -1.699) (end 2.961 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 51dceee2-16f6-43f7-8551-cd3dd85bdcc4))
    (fp_line (start 2.961 1.04) (end 2.961 1.699)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp aac2b8a2-27ec-4a74-bf95-ee17a17418bd))
    (fp_line (start 3.001 -1.653) (end 3.001 -1.04)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 64a031a3-a1ec-4901-b808-b885a44d23e1))
    (fp_line (start 3.001 1.04) (end 3.001 1.653)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2b67d6e7-2fc6-49e3-ad54-f212b38f81a7))
    (fp_line (start 3.041 -1.605) (end 3.041 1.605)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bd42b19b-7615-46e1-af96-f04b16cc4e9d))
    (fp_line (start 3.081 -1.554) (end 3.081 1.554)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dbd3261d-8c67-4069-be45-b03e93056267))
    (fp_line (start 3.121 -1.5) (end 3.121 1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d3cabff1-b0dc-41af-8a9f-a33abb58a7fb))
    (fp_line (start 3.161 -1.443) (end 3.161 1.443)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4bdba487-696c-4c14-b610-eb8445b65261))
    (fp_line (start 3.201 -1.383) (end 3.201 1.383)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6001771f-dc1b-4fb8-b904-f86466307703))
    (fp_line (start 3.241 -1.319) (end 3.241 1.319)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp dd093b64-824d-4976-b625-b888111948c5))
    (fp_line (start 3.281 -1.251) (end 3.281 1.251)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 45423e9d-d8f5-4422-af97-69492cc653d4))
    (fp_line (start 3.321 -1.178) (end 3.321 1.178)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 53e256ff-44a7-4057-a9f3-069e9fb5f9b7))
    (fp_line (start 3.361 -1.098) (end 3.361 1.098)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3bca68c0-66b5-46e6-8e79-536cd78f75d7))
    (fp_line (start 3.401 -1.011) (end 3.401 1.011)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 00045109-5913-4be1-b844-15e0dd7db124))
    (fp_line (start 3.441 -0.915) (end 3.441 0.915)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp acbedabf-5b23-4cd8-bb8e-c909cf6e64c0))
    (fp_line (start 3.481 -0.805) (end 3.481 0.805)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4c42b7ab-98ad-4402-b504-dc7d2d028700))
    (fp_line (start 3.521 -0.677) (end 3.521 0.677)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ecc761fa-09c7-4452-9619-36f525247d2d))
    (fp_line (start 3.561 -0.518) (end 3.561 0.518)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e62d514d-5449-4bfa-80a2-77a9bc706016))
    (fp_line (start 3.601 -0.284) (end 3.601 0.284)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp eaee9510-7950-4c8b-b52e-1a43d77d49e5))
    (fp_circle (center 1 0) (end 3.62 0)
      (stroke (width 0.12) (type solid)) (fill none) (layer "F.SilkS") (tstamp 7eddfe58-74b4-491a-889e-d1cbbe407bc2))
    (fp_circle (center 1 0) (end 3.75 0)
      (stroke (width 0.05) (type solid)) (fill none) (layer "F.CrtYd") (tstamp 0e370603-96f6-40b3-8a8c-87f13be52e16))
    (fp_line (start -1.133605 -1.0875) (end -0.633605 -1.0875)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 22a1a4f3-ca80-438b-b45f-3678536584b8))
    (fp_line (start -0.883605 -1.3375) (end -0.883605 -0.8375)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e9e08ce3-f979-4db7-a01f-1a941f544c8a))
    (fp_circle (center 1 0) (end 3.5 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 23b53cc8-b631-455a-ad1f-72c78675abfd))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive") (tstamp e26a36e0-7241-4390-8f94-78223ed2b022))
    (pad "2" thru_hole circle (at 2 0 90) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J2-Pin_1)") (pintype "passive") (tstamp e98487cc-3568-4473-924c-ee2dd8caf83f))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_D5.0mm_P2.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_DIP:DIP-8_W7.62mm" (layer "F.Cu")
    (tstamp 2fa7f398-fe07-4414-8e2c-675eeae49fff)
    (at 102.88 107.96)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (property "Sheetfile" "led-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, DIP-8")
    (property "ki_keywords" "AVR 8bit Microcontroller tinyAVR")
    (path "/cc4e7474-c0ce-4289-b3c6-7af942381fa0")
    (attr through_hole)
    (fp_text reference "U2" (at 3.81 -2.33) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 44d29630-7346-4acd-bd97-f819e71b7a64)
    )
    (fp_text value "ATtiny45-20P" (at 3.81 9.95) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 6c95fe55-4cf7-4428-b109-f8e6de595b2a)
    )
    (fp_text user "${REFERENCE}" (at 3.81 3.81) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f375b874-738c-41cc-a9d2-0f02b4a056c9)
    )
    (fp_line (start 1.16 -1.33) (end 1.16 8.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 52f59e6d-c541-4963-b417-43d69eebae06))
    (fp_line (start 1.16 8.95) (end 6.46 8.95)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp de95a92c-fd1a-4e45-b550-71c4d4779d0e))
    (fp_line (start 2.81 -1.33) (end 1.16 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 09985e62-ae77-4013-92d3-5d2ffca627e4))
    (fp_line (start 6.46 -1.33) (end 4.81 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ff87dc49-f822-4ac6-8d2d-48bfa6c9b043))
    (fp_line (start 6.46 8.95) (end 6.46 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 87efbe7f-2538-43a8-bdf7-33dfc540c1fa))
    (fp_arc (start 4.81 -1.33) (mid 3.81 -0.33) (end 2.81 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fa9f8e55-4a18-42ad-b873-15bbfde94964))
    (fp_line (start -1.1 -1.55) (end -1.1 9.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 0030d3f3-6137-4a69-9b78-30f466e8f267))
    (fp_line (start -1.1 9.15) (end 8.7 9.15)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 6ce6902a-d33e-4579-8189-2c64864d7e34))
    (fp_line (start 8.7 -1.55) (end -1.1 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 810019c3-4c99-4557-b518-082c863216a1))
    (fp_line (start 8.7 9.15) (end 8.7 -1.55)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b821d929-eb7f-4a6a-8349-621249a75a92))
    (fp_line (start 0.635 -0.27) (end 1.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 20317ac1-109d-400d-ae2e-48f863f0debb))
    (fp_line (start 0.635 8.89) (end 0.635 -0.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6528ec21-4a1c-4f07-8c74-14ac01716126))
    (fp_line (start 1.635 -1.27) (end 6.985 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5e9d6178-fd16-418e-9db7-cf49b80d5268))
    (fp_line (start 6.985 -1.27) (end 6.985 8.89)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8ca0e3ba-d55f-4ea2-83be-2a387d7c9bda))
    (fp_line (start 6.985 8.89) (end 0.635 8.89)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 63ac5c11-e6b0-450f-bfd8-1ce146a9a5c4))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(J2-Pin_6)") (pinfunction "~{RESET}/PB5") (pintype "bidirectional") (tstamp 38b2bd54-dc51-485c-a741-12bb0120a139))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 7 "unconnected-(U2-XTAL1{slash}PB3-Pad2)") (pinfunction "XTAL1/PB3") (pintype "bidirectional") (tstamp 6227f91b-47dd-4b65-9d73-01dd386037fe))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(Q3-G)") (pinfunction "XTAL2/PB4") (pintype "bidirectional") (tstamp 013a1319-7eba-429e-bff0-059051449343))
    (pad "4" thru_hole oval (at 0 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp f5aeb55a-8501-49ae-96b3-68f040dafc7c))
    (pad "5" thru_hole oval (at 7.62 7.62) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(J2-Pin_3)") (pinfunction "AREF/PB0") (pintype "bidirectional") (tstamp 09e38363-b5a7-4b78-86af-f8d2e39aa523))
    (pad "6" thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J2-Pin_4)") (pinfunction "PB1") (pintype "bidirectional") (tstamp f92c4cc9-5fe4-4f3f-966c-30718f7a4817))
    (pad "7" thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(J2-Pin_5)") (pinfunction "PB2") (pintype "bidirectional") (tstamp 5943af82-cbd3-48eb-80e4-63a71ae21988))
    (pad "8" thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J2-Pin_1)") (pinfunction "VCC") (pintype "power_in") (tstamp 00f82f41-47e0-4fac-b921-82cdf9461821))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (tstamp 45f1578e-d440-49f2-a2d3-cb9fd12dcad7)
    (at 104.14 101.6)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Sheetfile" "led-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Positive 1A 35V Linear Regulator, Fixed Output 5V, TO-220")
    (property "ki_keywords" "Voltage Regulator 1A Positive")
    (path "/14118208-d22c-401e-82d3-6e7cea3c6576")
    (attr through_hole)
    (fp_text reference "U1" (at 2.54 -4.27) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a5f492a0-ed63-44d6-9ac2-e3a6600fe376)
    )
    (fp_text value "LM7805_TO220" (at 2.54 2.5) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 540a4e4d-a3a1-48ce-a38b-762446b99d3e)
    )
    (fp_text user "${REFERENCE}" (at 2.54 -4.27) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp fcc6ed32-b356-488a-b5c9-f8407c80038a)
    )
    (fp_line (start -2.58 -3.27) (end -2.58 1.371)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f6c9ed42-b26a-4f70-bae5-3ac972fe815d))
    (fp_line (start -2.58 -3.27) (end 7.66 -3.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8fac2ff0-e19f-476c-96cc-1bdd20da5173))
    (fp_line (start -2.58 -1.76) (end 7.66 -1.76)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 97e7b4b9-891c-41bb-a2a5-d91e82b51a17))
    (fp_line (start -2.58 1.371) (end 7.66 1.371)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2ea99d03-4560-45f9-8f6c-aa971c2bd07a))
    (fp_line (start 0.69 -3.27) (end 0.69 -1.76)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp fbd61989-75f3-4dd9-9399-0d26b997b362))
    (fp_line (start 4.391 -3.27) (end 4.391 -1.76)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cad53296-257b-4ae5-984d-57715e8e836f))
    (fp_line (start 7.66 -3.27) (end 7.66 1.371)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 42c7be10-0651-40ab-b68a-0bf385a57e25))
    (fp_line (start -2.71 -3.4) (end -2.71 1.51)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp fa043b65-a50b-4ecc-beff-847e1ecf78c3))
    (fp_line (start -2.71 1.51) (end 7.79 1.51)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 2e6acc0d-ebec-499d-97f9-b51b8b63ba95))
    (fp_line (start 7.79 -3.4) (end -2.71 -3.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 38f2f3c7-d095-472c-b1ce-75e3eb171600))
    (fp_line (start 7.79 1.51) (end 7.79 -3.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 472bb8b7-3142-4350-9812-71c8b2ddf794))
    (fp_line (start -2.46 -3.15) (end -2.46 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp af13cfda-9036-41ce-9f84-e3858a72feda))
    (fp_line (start -2.46 -1.88) (end 7.54 -1.88)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6dd90304-f348-45f8-a67f-fd264fceb01d))
    (fp_line (start -2.46 1.25) (end 7.54 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e4d143be-e86f-43b2-9be0-7fbeecb72cd4))
    (fp_line (start 0.69 -3.15) (end 0.69 -1.88)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2e6b6829-51ba-4d78-8540-231819afca6b))
    (fp_line (start 4.39 -3.15) (end 4.39 -1.88)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1c4ee764-d255-4cbc-8996-d485032b7648))
    (fp_line (start 7.54 -3.15) (end -2.46 -3.15)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f7a374ae-bd1d-4efa-967f-5404dcfd6b8a))
    (fp_line (start 7.54 1.25) (end 7.54 -3.15)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0e87e472-5f9c-4f95-bd88-7c9dca880d9c))
    (pad "1" thru_hole rect (at 0 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(BT1-+)") (pinfunction "VI") (pintype "power_in") (tstamp b211dc9b-ffdd-4364-930e-17ef62a1eb5a))
    (pad "2" thru_hole oval (at 2.54 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "GND") (pintype "power_in") (tstamp f48d6512-ca96-4e0d-8b66-6cde645af0fb))
    (pad "3" thru_hole oval (at 5.08 0) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J2-Pin_1)") (pinfunction "VO") (pintype "power_out") (tstamp 7b4b4a85-0bb3-420d-93c7-e76f89a3ce84))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tstamp 638b682d-0078-46b1-8a79-66609c2b5eef)
    (at 76.2 96.52 -90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Feld4" "")
    (property "Sheetfile" "led-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/304b0b82-58bd-438d-a5d7-69c727691bf3")
    (attr through_hole)
    (fp_text reference "R3" (at 3.81 -1.92 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 4d89666c-aae5-4568-85b7-fde85d6d781d)
    )
    (fp_text value "100k" (at 3.81 1.92 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp cbcbc1c2-7b20-4543-aa96-5d20aea7c6a3)
    )
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab")
        (effects (font (size 0.72 0.72) (thickness 0.108)))
      (tstamp eb7bd6f3-c600-46e5-81ca-02e9d91b22d1)
    )
    (fp_line (start 0.94 0) (end 1.89 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 478779b5-d015-476d-997b-b3afe9edb04b))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b11bcd3e-f281-4630-b6e0-da2976e12d04))
    (fp_line (start 1.89 0.92) (end 5.73 0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8b744d0a-34a4-49dc-928b-849f2cfb68fd))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2ea2fee4-ac77-4596-a9c3-38526983a2ac))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp d76a0c7f-8898-41b5-8ffa-a4b2d493cc34))
    (fp_line (start 6.68 0) (end 5.73 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f034a03c-75bd-4c76-bad4-57240db07809))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 28a1a8d5-1905-45db-adbd-58ca8d94c59f))
    (fp_line (start -0.95 1.05) (end 8.57 1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 83030343-4119-41ff-a644-be8b5723ee04))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 43e68e57-66c8-4ef5-a0b4-b6e33d5be9b1))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 8f87492e-4362-4579-9419-a0206d63dddd))
    (fp_line (start 0 0) (end 2.01 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f16d06cd-e19b-4413-895e-c2f535aa45c0))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5b71dcef-8792-4673-a03c-841be23ea7de))
    (fp_line (start 2.01 0.8) (end 5.61 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e83ded1a-09e5-4bb1-87fc-a1a5e6c06ac3))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 73e9f9c2-5fa0-4279-bd25-3cfd0bfbb0a6))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 859abbb1-8413-4266-8ccf-8017de6c7e57))
    (fp_line (start 7.62 0) (end 5.61 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 19ed8e25-c4ac-4671-905e-e761e0703f77))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(Q3-G)") (pintype "passive") (tstamp 463b6320-31d4-4b8a-9c59-ac5e7323a0fe))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive") (tstamp 429f962c-3434-4619-bda2-bf33a42aa51d))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Connector_PinHeader_2.54mm:PinHeader_1x06_P2.54mm_Vertical" (layer "F.Cu")
    (tstamp 65685b0a-7661-4dc8-ba35-8b438ab8f725)
    (at 114.3 115.57 180)
    (descr "Through hole straight pin header, 1x06, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x06 2.54mm single row")
    (property "Sheetfile" "led-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x06, script generated")
    (property "ki_keywords" "connector")
    (path "/ccc2476a-3d91-4d08-9b99-901f9f21b284")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 14eb4dde-e85d-4bb0-8cd2-5f4185549e41)
    )
    (fp_text value "Conn_01x06_Socket" (at 0 15.03) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp f71435fb-4f52-4a43-82c8-8b821cdbfef3)
    )
    (fp_text user "${REFERENCE}" (at 0 6.35 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 12cd8979-6bc8-4c8d-831a-d6d4b8163510)
    )
    (fp_line (start -1.33 -1.33) (end 0 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 84768567-8dc3-4832-a431-521eafb205f6))
    (fp_line (start -1.33 0) (end -1.33 -1.33)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2bab00c6-60a1-465a-a1e9-37ebc510eb6e))
    (fp_line (start -1.33 1.27) (end -1.33 14.03)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 69e1d444-27eb-4a6e-b4a5-46cd513ec877))
    (fp_line (start -1.33 1.27) (end 1.33 1.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b67aaac7-090c-4c78-87c0-aa05c7208943))
    (fp_line (start -1.33 14.03) (end 1.33 14.03)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0586aaa7-acf7-498e-a47d-4c259cd246fc))
    (fp_line (start 1.33 1.27) (end 1.33 14.03)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2ce916a0-84f4-41c1-9b10-c29b2232da4e))
    (fp_line (start -1.8 -1.8) (end -1.8 14.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 964ee3ed-dc2d-4bbc-a6c7-5dc71df657df))
    (fp_line (start -1.8 14.5) (end 1.8 14.5)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5e47e16b-9fe9-4818-89f0-4cd741f65ebe))
    (fp_line (start 1.8 -1.8) (end -1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 1ca619cc-548c-43ac-a03b-1c80141076e4))
    (fp_line (start 1.8 14.5) (end 1.8 -1.8)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 63980e53-273f-4f13-82ce-79feb438e7cd))
    (fp_line (start -1.27 -0.635) (end -0.635 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 14ad99dd-0e63-4054-b5f8-f80955eb90eb))
    (fp_line (start -1.27 13.97) (end -1.27 -0.635)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 29cda9f4-8fd7-4cf6-99df-d85e57ba6257))
    (fp_line (start -0.635 -1.27) (end 1.27 -1.27)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cadc6efe-2d78-4569-9941-06d09d317164))
    (fp_line (start 1.27 -1.27) (end 1.27 13.97)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d639c25a-eda4-4e7e-91f1-dbe91f701a86))
    (fp_line (start 1.27 13.97) (end -1.27 13.97)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4279678d-ddb7-4241-9a6c-62e882a1e63c))
    (pad "1" thru_hole rect (at 0 0 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 8 "Net-(J2-Pin_1)") (pinfunction "Pin_1") (pintype "passive") (tstamp f62d68b3-fa49-4e12-9ba6-51c3a0288d3b))
    (pad "2" thru_hole oval (at 0 2.54 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "Pin_2") (pintype "passive") (tstamp d8d10b97-e5bc-4122-86e8-29beef3a6afe))
    (pad "3" thru_hole oval (at 0 5.08 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(J2-Pin_3)") (pinfunction "Pin_3") (pintype "passive") (tstamp fdd2187d-3779-45bb-83a1-ccb0c046f645))
    (pad "4" thru_hole oval (at 0 7.62 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J2-Pin_4)") (pinfunction "Pin_4") (pintype "passive") (tstamp 7a658cc9-eb9c-494a-a05e-4de7da545789))
    (pad "5" thru_hole oval (at 0 10.16 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 11 "Net-(J2-Pin_5)") (pinfunction "Pin_5") (pintype "passive") (tstamp aa004b1a-9d45-4c6b-a669-375cc3205760))
    (pad "6" thru_hole oval (at 0 12.7 180) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 12 "Net-(J2-Pin_6)") (pinfunction "Pin_6") (pintype "passive") (tstamp 7fb76073-1fbb-4627-8c53-b08fbde8bf88))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x06_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tstamp 6e9df83c-66b6-423e-b0fc-288e573f8571)
    (at 86.36 96.52 -90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "led-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/267fb370-609d-4c7e-8bd4-8b6ac6591673")
    (attr through_hole)
    (fp_text reference "R2" (at 3.81 -1.92 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e1201ef3-3bc4-42fa-ad98-86d916cc6e65)
    )
    (fp_text value "100k" (at 3.81 1.92 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 74137c7d-0889-473f-a2fc-22cba260f800)
    )
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab")
        (effects (font (size 0.72 0.72) (thickness 0.108)))
      (tstamp 42e3cd17-e744-427a-bad1-2bd125bc58ac)
    )
    (fp_line (start 0.94 0) (end 1.89 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e11e1069-4089-445d-b6cd-841bc7d4c4a5))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 02e32672-74aa-4168-b2f4-79a45d3f647b))
    (fp_line (start 1.89 0.92) (end 5.73 0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e7f08404-a1d6-4d16-a576-d94d5c226b83))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 58661e1c-880a-4ca9-8eac-92813292cbca))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a04447b1-7356-407e-93d1-abf07656f7c5))
    (fp_line (start 6.68 0) (end 5.73 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f04df38d-92b8-47db-b2b6-ddebd833015c))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5de03b3b-1480-4b5b-b100-5ef8d39bcf06))
    (fp_line (start -0.95 1.05) (end 8.57 1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ba283cf5-0657-4289-91ba-cb61fee6dcd7))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7fbf914b-8835-484f-b8ed-d0a1cff1fc30))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 511ecf52-d6cd-4039-8c0e-f4ac00ae2fe0))
    (fp_line (start 0 0) (end 2.01 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 70c4bf3b-d303-4d0b-be7d-b42291c097df))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c313ddc1-b22a-403c-b6a8-6a255ceddec9))
    (fp_line (start 2.01 0.8) (end 5.61 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 25373c79-2718-41f1-bed6-96867a190168))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 964cadbb-9eb5-473d-a2ea-cd0990d6a921))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 939cc135-98b8-4d1c-9ed2-e8c13eff4d1d))
    (fp_line (start 7.62 0) (end 5.61 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2930e795-21fd-49c1-b48a-b60d76530335))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 10 "Net-(J2-Pin_4)") (pintype "passive") (tstamp 1ca0f3fb-3155-4e02-9241-bcc9ef8ba54b))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive") (tstamp 2d207a38-f452-465c-9619-06a41de04496))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Resistor_THT:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (tstamp 7401d5f0-600f-4d6b-87a1-6982f58d4696)
    (at 96.52 96.52 -90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "led-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor")
    (property "ki_keywords" "R res resistor")
    (path "/90dbdc91-46c9-4b01-b3fc-3a001184cea4")
    (attr through_hole)
    (fp_text reference "R1" (at 3.81 -1.92 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 783cb14a-a8d4-45a5-a0aa-417201838a87)
    )
    (fp_text value "100k" (at 3.81 1.92 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 13253ffa-4d7d-4a3f-b160-7ba5059aef40)
    )
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab")
        (effects (font (size 0.72 0.72) (thickness 0.108)))
      (tstamp 72a9fc9b-9c45-4172-af2f-026be7493b2a)
    )
    (fp_line (start 0.94 0) (end 1.89 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 42b6d542-c846-440a-82f4-789265a83765))
    (fp_line (start 1.89 -0.92) (end 1.89 0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2b746f5d-f046-4848-a87f-e1374aa27e72))
    (fp_line (start 1.89 0.92) (end 5.73 0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 4ae0e48c-f6df-4027-80a7-1e10b0155f0a))
    (fp_line (start 5.73 -0.92) (end 1.89 -0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 2f06c727-d1df-459c-bd32-04d6e62f2029))
    (fp_line (start 5.73 0.92) (end 5.73 -0.92)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7a7bc587-d041-4776-8fca-1b4e4dee0a78))
    (fp_line (start 6.68 0) (end 5.73 0)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 30a2068d-550e-40fd-ad84-e8360d701b2c))
    (fp_line (start -0.95 -1.05) (end -0.95 1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp b600ec49-4e18-4b47-a195-29656902e2df))
    (fp_line (start -0.95 1.05) (end 8.57 1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp af74c7a5-13b1-4e80-9345-991c09fa1930))
    (fp_line (start 8.57 -1.05) (end -0.95 -1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 81c9a18c-3b2a-431a-bd2f-8391d322ef8a))
    (fp_line (start 8.57 1.05) (end 8.57 -1.05)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f688e081-d533-4c65-be70-6c6abcf86ce2))
    (fp_line (start 0 0) (end 2.01 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 45c3c49b-d0fb-4a09-bb76-2158eca27ad1))
    (fp_line (start 2.01 -0.8) (end 2.01 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 15a09709-0c74-4df9-afdf-59331d2068f1))
    (fp_line (start 2.01 0.8) (end 5.61 0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 67fd3202-ac62-41c6-9431-7dabd3c533db))
    (fp_line (start 5.61 -0.8) (end 2.01 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7c41d2c7-c9cf-4c26-b332-2cb65cba338d))
    (fp_line (start 5.61 0.8) (end 5.61 -0.8)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 58e2a8e6-8947-4bf9-8ffd-c4f487b2197e))
    (fp_line (start 7.62 0) (end 5.61 0)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f3f9448e-adfe-434f-a7df-b51623a5ae4b))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(J2-Pin_3)") (pintype "passive") (tstamp 0c8688f4-0c7f-4ec1-9d2b-f36284aa3468))
    (pad "2" thru_hole oval (at 7.62 0 270) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pintype "passive") (tstamp 3b75e2a5-a571-4b12-bd2e-7cc4e2bc93b0))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TerminalBlock_TE-Connectivity:TerminalBlock_TE_282834-4_1x04_P2.54mm_Horizontal" (layer "F.Cu")
    (tstamp 75756c00-b1b8-4f63-b710-e816d1bf05f1)
    (at 83.82 111.76 180)
    (descr "Terminal Block TE 282834-4, 4 pins, pitch 2.54mm, size 10.620000000000001x6.5mm^2, drill diamater 1.1mm, pad diameter 2.1mm, see http://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F282834%7FC1%7Fpdf%7FEnglish%7FENG_CD_282834_C1.pdf, script-generated using https://github.com/pointhi/kicad-footprint-generator/scripts/TerminalBlock_TE-Connectivity")
    (tags "THT Terminal Block TE 282834-4 pitch 2.54mm size 10.620000000000001x6.5mm^2 drill 1.1mm pad 2.1mm")
    (property "Sheetfile" "led-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Generic connector, single row, 01x04, script generated")
    (property "ki_keywords" "connector")
    (path "/69d099f9-9098-463f-8369-284ce5d555c2")
    (attr through_hole)
    (fp_text reference "J1" (at 3.81 -4.37) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 04d07af4-5601-4c6f-b68f-e5d5c88079e8)
    )
    (fp_text value "+12V_STRIP" (at 3.81 4.37) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp e5c16a1b-ea3f-4509-a638-94233ebed63f)
    )
    (fp_text user "${REFERENCE}" (at 3.81 2) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a414f91e-87b3-403f-ba3b-6a00e4b2d5a7)
    )
    (fp_line (start -1.86 2.97) (end -1.86 3.61)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp e6177ff1-cac3-4253-9af2-e1ada2ef98d3))
    (fp_line (start -1.86 3.61) (end -1.46 3.61)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8efb09f5-d7ba-4b6f-86ea-22c70ee9c2d6))
    (fp_line (start -1.62 -3.37) (end -1.62 3.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8d9d7547-02be-4605-b29a-1e4a3bbf44a7))
    (fp_line (start -1.62 -3.37) (end 9.241 -3.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 5f512801-e1bd-4731-a5a6-ad37a0f0649f))
    (fp_line (start -1.62 -2.25) (end 9.241 -2.25)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 1dcf7136-169c-4c9d-a4f4-28dfa1a63664))
    (fp_line (start -1.62 2.85) (end 9.241 2.85)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 93c6920a-8c08-42e8-9136-757fbf9e39d0))
    (fp_line (start -1.62 3.37) (end 9.241 3.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 553163c6-fe63-4fca-9627-5b21e6406070))
    (fp_line (start 9.241 -3.37) (end 9.241 3.37)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp bdbfa24b-374a-4f06-8d01-2e195cb80ae3))
    (fp_line (start -2 -3.75) (end -2 3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 5a6877e0-70c9-4d8a-b117-9e23908005e7))
    (fp_line (start -2 3.75) (end 9.63 3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 9fb13903-a5b9-4b6e-b611-cb0f61eb8a5f))
    (fp_line (start 9.63 -3.75) (end -2 -3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp e250cff0-c70a-432b-a727-8168449a32aa))
    (fp_line (start 9.63 3.75) (end 9.63 -3.75)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 44c7da23-8e17-4f21-918c-3e791d311975))
    (fp_line (start -1.5 -3.25) (end 9.12 -3.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2f3d0271-1792-4fd8-8301-bfe83cfe24bd))
    (fp_line (start -1.5 -2.25) (end 9.12 -2.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9fb6cd6c-366e-4532-ae19-4a881f6894c2))
    (fp_line (start -1.5 2.85) (end -1.5 -3.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4e8d446c-ae94-40ae-906a-9ed60e158fa2))
    (fp_line (start -1.5 2.85) (end 9.12 2.85)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8a8f8b1f-a42c-41a2-8280-1d7cfc60f7fb))
    (fp_line (start -1.1 3.25) (end -1.5 2.85)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 664ffd06-76bf-4a02-a565-07979e3ca01e))
    (fp_line (start 0.701 -0.835) (end -0.835 0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0a81756d-0d48-4237-9b45-de9457de96fd))
    (fp_line (start 0.835 -0.7) (end -0.701 0.835)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 210ce43c-8cc0-40c7-9eab-4926271f9ec3))
    (fp_line (start 3.241 -0.835) (end 1.706 0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4c5a39ed-be69-4b14-9cdb-a69a0f74e304))
    (fp_line (start 3.375 -0.7) (end 1.84 0.835)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 37102ecb-89ac-4ccc-8f51-64e43466881c))
    (fp_line (start 5.781 -0.835) (end 4.246 0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 46964d96-d042-4ed2-a102-a46fd7acf666))
    (fp_line (start 5.915 -0.7) (end 4.38 0.835)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 56b9d0e5-cf70-460c-9e9b-d4c5ca59aca5))
    (fp_line (start 8.321 -0.835) (end 6.786 0.7)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 02b4955d-86e5-48cd-8a7a-c7a8a29cf095))
    (fp_line (start 8.455 -0.7) (end 6.92 0.835)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3a2133f5-90fa-4195-bbf5-c406d230044e))
    (fp_line (start 9.12 -3.25) (end 9.12 3.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp ea394ef1-3fca-4a2d-b8ff-75979bbabe0a))
    (fp_line (start 9.12 3.25) (end -1.1 3.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9f5f0d61-3a3a-4279-9a47-04b58c6d134c))
    (fp_circle (center 0 0) (end 1.1 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 244153ba-cecd-45eb-ba6b-069c02eb3f10))
    (fp_circle (center 2.54 0) (end 3.64 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 78e17422-4c09-4d12-9b93-455f64e68f5e))
    (fp_circle (center 5.08 0) (end 6.18 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 0808c8cf-b8c5-4044-9143-1925fcdf13d9))
    (fp_circle (center 7.62 0) (end 8.72 0)
      (stroke (width 0.1) (type solid)) (fill none) (layer "F.Fab") (tstamp 123f43d6-af62-4ec8-ae9b-f28786bdb624))
    (pad "1" thru_hole rect (at 0 0 180) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(BT1-+)") (pinfunction "Pin_1") (pintype "passive") (tstamp 66eb89f9-da83-4b9a-9398-4584b5ee04fc))
    (pad "2" thru_hole circle (at 2.54 0 180) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(J1-Pin_2)") (pinfunction "Pin_2") (pintype "passive") (tstamp 6b17ebd4-33f0-4597-9859-ffc2a66d99b6))
    (pad "3" thru_hole circle (at 5.08 0 180) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 3 "Net-(J1-Pin_3)") (pinfunction "Pin_3") (pintype "passive") (tstamp 9e7a878e-f1ab-4c06-bca7-3762377feefa))
    (pad "4" thru_hole circle (at 7.62 0 180) (size 2.1 2.1) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J1-Pin_4)") (pinfunction "Pin_4") (pintype "passive") (tstamp 54f74844-f2b6-411d-a7d6-db4e255320a3))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock_TE-Connectivity.3dshapes/TerminalBlock_TE_282834-4_1x04_P2.54mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "TerminalBlock:TerminalBlock_Altech_AK300-2_P5.00mm" (layer "F.Cu")
    (tstamp 9c632806-6b46-4978-b397-2e9c2514b0b9)
    (at 104.22 88.9)
    (descr "Altech AK300 terminal block, pitch 5.0mm, 45 degree angled, see http://www.mouser.com/ds/2/16/PCBMETRC-24178.pdf")
    (tags "Altech AK300 terminal block pitch 5.0mm")
    (property "Sheetfile" "led-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Multiple-cell battery")
    (property "ki_keywords" "batt voltage-source cell")
    (path "/dda22bd2-68a2-4e19-bd3c-f7e3c075b9ca")
    (attr through_hole)
    (fp_text reference "BT1" (at -1.92 -6.99) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 34c29f91-98b7-4e98-822d-45fc875a4367)
    )
    (fp_text value "B12V" (at 2.78 7.75) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp a958c20f-0e14-44a8-8ba5-99fdd11894dc)
    )
    (fp_text user "${REFERENCE}" (at 2.5 -2) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 5bb1c603-eb4b-423d-ae7c-2fae7160f1b3)
    )
    (fp_line (start -2.65 -6.3) (end -2.65 6.3)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 6ed5c804-614e-456c-b86b-c8ba98c35102))
    (fp_line (start -2.65 6.3) (end 7.7 6.3)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 50fa9160-edba-4dc4-90b7-b4c4af94716a))
    (fp_line (start 7.7 -1.5) (end 8.2 -1.2)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp ad3ea20a-9682-43d8-9693-ca0eac5d268a))
    (fp_line (start 7.7 3.9) (end 7.7 -1.5)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 7cb3ec8e-d2b9-429b-a035-ef968897d5af))
    (fp_line (start 7.7 5.35) (end 8.2 5.6)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 817a0e4f-e446-4ff6-82a8-56abc5cf5b57))
    (fp_line (start 7.7 6.3) (end 7.7 5.35)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 0ad6b5b2-53da-4934-9b6f-352f53befaa4))
    (fp_line (start 8.2 -6.3) (end -2.65 -6.3)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 598ece30-116a-48f6-bc85-e76ecbf88167))
    (fp_line (start 8.2 -1.2) (end 8.2 -6.3)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a55f4ba0-0574-45dc-af40-73d8d1848999))
    (fp_line (start 8.2 3.65) (end 7.7 3.9)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 3d659603-d033-4b11-8e45-4088330defd6))
    (fp_line (start 8.2 3.7) (end 8.2 3.65)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp baae968f-ece0-412f-802c-b571009b23b9))
    (fp_line (start 8.2 5.6) (end 8.2 3.7)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b8249b7b-8fb5-4c03-9e8e-cccca072e709))
    (fp_line (start -2.83 -6.47) (end -2.83 6.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 4862a369-4adc-4e39-bf71-9e8b4348abd6))
    (fp_line (start -2.83 -6.47) (end 8.36 -6.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp cfd132da-799e-44a8-84b4-01a0e016b942))
    (fp_line (start 8.36 6.47) (end -2.83 6.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp a7763f26-ce7b-48c3-84af-0728a6a7f655))
    (fp_line (start 8.36 6.47) (end 8.36 -6.47)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 477cfc9f-9a85-4367-bc44-2d6594b9c793))
    (fp_line (start -2.58 -3.17) (end -2.58 -6.22)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8371740e-e0ca-4a30-8564-d7ae08b1854a))
    (fp_line (start -2.58 -3.17) (end 7.61 -3.17)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c1c308b5-2c28-454e-bc54-03ad430c7385))
    (fp_line (start -2.58 -0.64) (end -2.58 -3.17)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4e298545-76ef-4275-9e3b-91c41b5a7275))
    (fp_line (start -2.58 -0.64) (end -1.64 -0.64)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9f3adb04-eef4-4a68-8339-ed152316894f))
    (fp_line (start -2.58 6.22) (end -2.58 -0.64)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8793f106-e29d-4be8-9780-3d4847503621))
    (fp_line (start -2.58 6.22) (end -2.02 6.22)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7b5cadb2-276a-407b-879d-a1a3cc3eb846))
    (fp_line (start -2.02 -3.43) (end -2.02 -5.97)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5037c137-38e0-4870-bb55-4404346a4d21))
    (fp_line (start -2.02 -0.25) (end -2.02 4.32)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e71e513c-f6f8-4ae8-a576-248a246b4e4d))
    (fp_line (start -2.02 -0.25) (end -1.64 -0.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f841a6a8-4adb-4ce0-8ab4-4a204a795559))
    (fp_line (start -2.02 4.32) (end -2.02 6.22)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 89f48848-70b7-4583-b756-8c6d51825721))
    (fp_line (start -2.02 6.22) (end 2.04 6.22)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c05a7ad4-59e5-4726-8592-4016df436ff8))
    (fp_line (start -1.64 -0.64) (end 1.66 -0.64)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fd21c457-80ef-4f84-b099-3adeeed0a834))
    (fp_line (start -1.64 0.51) (end -1.26 0.51)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 90d4dc73-b1a0-44f8-b6d2-500d1151e59a))
    (fp_line (start -1.64 3.68) (end -1.64 0.51)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d54e7ccf-2a61-4cd7-a27d-28b837314489))
    (fp_line (start -1.62 -4.45) (end 1.44 -5.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6d6a85a8-d4c3-428b-8ba6-b742d92ada71))
    (fp_line (start -1.49 -4.32) (end 1.56 -4.95)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bcee40a5-c6c4-4d38-8dc2-213aa5cb2717))
    (fp_line (start -1.26 -0.25) (end 1.28 -0.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3d5f6938-53b1-4b36-b106-35698d5e2ffe))
    (fp_line (start -1.26 2.54) (end -1.26 -0.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 367427f5-f1e6-46bb-a0bd-1e2ec7af0ef1))
    (fp_line (start -1.26 2.54) (end 1.28 2.54)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 0b160ac8-2a02-4106-933c-821bdadc4d5a))
    (fp_line (start 1.28 2.54) (end 1.28 -0.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fbac7cb0-298f-4452-91cf-259b766e95cd))
    (fp_line (start 1.66 -0.64) (end 3.36 -0.64)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e9f59268-25d4-49f2-bb3a-319ba05cbfc3))
    (fp_line (start 1.66 -0.25) (end -1.64 -0.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8c76e0b3-5acf-48c1-ac78-af9b3bd53fee))
    (fp_line (start 1.66 0.51) (end 1.28 0.51)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8a1cfa6d-62f1-4fd6-bc27-f1bab52b94b4))
    (fp_line (start 1.66 3.68) (end -1.64 3.68)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 06e3b0a1-35f2-44da-807a-8cc3b60a5381))
    (fp_line (start 1.66 3.68) (end 1.66 0.51)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9f60941b-daef-4091-a1e5-16ad10843b07))
    (fp_line (start 2.04 -5.97) (end -2.02 -5.97)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d2bc3103-e76f-4ab9-8013-629241878089))
    (fp_line (start 2.04 -3.43) (end -2.02 -3.43)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9645fc2e-abb6-4dd8-ab90-beb2244280a7))
    (fp_line (start 2.04 -3.43) (end 2.04 -5.97)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b35ff119-6a69-4160-9cc3-8fd7b3b874ee))
    (fp_line (start 2.04 -0.25) (end 1.66 -0.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d00323b6-11c2-402e-8561-05cf71eb2529))
    (fp_line (start 2.04 4.32) (end -2.02 4.32)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bad68caf-810e-4ee2-979a-4855d842c16b))
    (fp_line (start 2.04 4.32) (end 2.04 -0.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 110d9a7f-d713-4527-9b1c-c7f63ab9d54e))
    (fp_line (start 2.04 6.22) (end 2.04 4.32)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 30061278-209c-4e7a-ac47-808915ed6c54))
    (fp_line (start 2.04 6.22) (end 2.98 6.22)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5f9faf70-3b75-48c8-bb35-ad704783efe8))
    (fp_line (start 2.98 -5.97) (end 7.05 -5.97)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8161c720-d453-476d-b90d-7148ab9cf2e3))
    (fp_line (start 2.98 -3.43) (end 2.98 -5.97)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp b407fcd2-a71a-42b1-94e2-0f1e81c16d71))
    (fp_line (start 2.98 -0.25) (end 3.36 -0.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a077e7f6-7b1d-4bed-b781-f6ae0e338d23))
    (fp_line (start 2.98 4.32) (end 2.98 -0.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 5ed3306c-cf60-4fb1-b96b-f25d31dd4c20))
    (fp_line (start 2.98 4.32) (end 7.05 4.32)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 49974b83-9a1a-4132-ab7b-b637521468d3))
    (fp_line (start 2.98 6.22) (end 2.98 4.32)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 417bee95-a369-4d2f-9776-bf922e721ab7))
    (fp_line (start 2.98 6.22) (end 7.05 6.22)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4223d536-5773-487a-93bb-9d947e2f12b1))
    (fp_line (start 3.36 -0.25) (end 6.67 -0.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 58bcafc8-e959-4fc7-9466-0e60044e053b))
    (fp_line (start 3.36 0.51) (end 3.74 0.51)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 158397c5-ccf0-4d4c-af07-2e58926244fb))
    (fp_line (start 3.36 3.68) (end 3.36 0.51)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e5966f07-52bb-452f-8d0f-456d776118bd))
    (fp_line (start 3.39 -4.45) (end 6.44 -5.08)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4cab474b-9065-45e3-ae3e-eb780cb1223f))
    (fp_line (start 3.52 -4.32) (end 6.56 -4.95)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9eb7745d-8770-4b69-8eae-4c6cd37c7c69))
    (fp_line (start 3.74 -0.25) (end 6.28 -0.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 7cca55c2-26c7-449d-999e-d3dcb39c07d9))
    (fp_line (start 3.74 2.54) (end 3.74 -0.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp bddaf88f-3d17-45f3-99dd-833bd3ea7671))
    (fp_line (start 3.74 2.54) (end 6.28 2.54)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 27d3b7aa-4e6b-4bca-9d12-e1dae96278cb))
    (fp_line (start 6.28 2.54) (end 6.28 -0.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp afbc0678-8b96-4b57-a773-bdda6d38d3f5))
    (fp_line (start 6.67 -0.64) (end 3.36 -0.64)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 61968f20-de20-45fc-894b-5a43b32bab33))
    (fp_line (start 6.67 0.51) (end 6.28 0.51)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp eb7f28d0-0f04-4bf4-9640-9f583fdd1168))
    (fp_line (start 6.67 3.68) (end 3.36 3.68)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3217f123-c5ba-4b7f-90a7-fe8546944885))
    (fp_line (start 6.67 3.68) (end 6.67 0.51)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1e8fa97b-a059-4bcb-9def-9ff882b82646))
    (fp_line (start 7.05 -5.97) (end 7.05 -3.43)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 570b0c72-c558-493d-bd5e-fa076b6ff508))
    (fp_line (start 7.05 -3.43) (end 2.98 -3.43)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp efe34a21-993a-4754-9fb4-eb01a44f16c1))
    (fp_line (start 7.05 -0.25) (end 6.67 -0.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp eba7812d-0399-4763-a3f4-fd24cb7ef2d4))
    (fp_line (start 7.05 -0.25) (end 7.05 4.32)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2bde614c-e5fc-41b3-961a-7ed34c3db149))
    (fp_line (start 7.05 4.32) (end 7.05 6.22)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp aa691d5c-98b7-4b67-8c70-96c1356c3402))
    (fp_line (start 7.05 6.22) (end 7.61 6.22)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3b191a5c-d35b-4db8-b9ff-2aa83b8e8853))
    (fp_line (start 7.61 -6.22) (end -2.58 -6.22)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a1eb2fb5-60ec-487a-b10e-822965e09188))
    (fp_line (start 7.61 -6.22) (end 7.61 -3.17)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 86ca4595-9370-46f1-b483-2c709381271e))
    (fp_line (start 7.61 -6.22) (end 8.11 -6.22)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 3e40f710-2666-4d8a-86b1-d5ad4ca47a2c))
    (fp_line (start 7.61 -3.17) (end 7.61 -1.65)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 765eb64f-0ce2-481b-bd62-a375364efe28))
    (fp_line (start 7.61 -1.65) (end 7.61 -0.64)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp cb4c48a8-d4e2-4cfb-bdfa-c14dc36fa072))
    (fp_line (start 7.61 -0.64) (end 6.67 -0.64)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 31873d82-7ac6-415f-b5f3-165b1b2c62f3))
    (fp_line (start 7.61 -0.64) (end 7.61 4.06)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6743403f-55cc-41f6-9da5-286f1d91e3a1))
    (fp_line (start 7.61 4.06) (end 7.61 5.21)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9343b39c-3a9c-4fb3-8143-c7bc67413ba1))
    (fp_line (start 7.61 5.21) (end 7.61 6.22)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp f442ca2d-45da-492d-a543-85692b03a927))
    (fp_line (start 8.11 -6.22) (end 8.11 -1.4)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 38046375-c8bc-4e15-8d85-4a4867236e28))
    (fp_line (start 8.11 -1.4) (end 7.61 -1.65)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fe4d4846-9929-4fb8-8571-4c11076e0f4c))
    (fp_line (start 8.11 3.81) (end 7.61 4.06)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c85c1d98-240b-4c98-9d65-2fe96abb0c0a))
    (fp_line (start 8.11 3.81) (end 8.11 5.46)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 40eee14c-4fa4-4528-a5c0-53865fbbfad5))
    (fp_line (start 8.11 5.46) (end 7.61 5.21)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp fb3f351c-18e4-4ab0-b312-1db742e8faec))
    (fp_arc (start -1.62 -5) (mid -0.05669 -5.772528) (end 1.539976 -5.071534)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 94fddb8c-7fd4-4877-a1b6-d24363495d87))
    (fp_arc (start -1.42 -4.13) (mid -1.718466 -4.559406) (end -1.562972 -5.058699)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2cd55029-fbbb-46fb-8d5c-5be029410c04))
    (fp_arc (start 1.53 -5.05) (mid 1.708693 -4.558754) (end 1.485619 -4.086005)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp c1df5f19-5617-4a05-a9cc-82cf3467ebb7))
    (fp_arc (start 1.53 -4.12) (mid 0.02849 -3.628196) (end -1.459829 -4.158582)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1d363848-2d26-48cd-93e6-a81ed184f0e3))
    (fp_arc (start 3.39 -5) (mid 4.949737 -5.764867) (end 6.538239 -5.061686)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9f907486-45ae-4d06-b2a3-9a98032aa9d1))
    (fp_arc (start 3.58 -4.13) (mid 3.281534 -4.559406) (end 3.437028 -5.058699)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 16da06d5-51b2-4155-b835-3ab1ee71264c))
    (fp_arc (start 6.53 -4.12) (mid 5.030583 -3.634318) (end 3.547667 -4.168263)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 57e0d509-2345-4aa9-8edf-64a73d8d6e42))
    (fp_arc (start 6.54 -5.05) (mid 6.715733 -4.551652) (end 6.485532 -4.076005)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2b294b81-fe31-4f52-9434-e46de417eb03))
    (pad "1" thru_hole rect (at 0 0) (size 1.98 3.96) (drill 1.32) (layers "*.Cu" "*.Mask")
      (net 6 "Net-(BT1-+)") (pinfunction "+") (pintype "passive") (tstamp 276cb00a-7287-4eef-bd02-2df61e8e69a1))
    (pad "2" thru_hole oval (at 5 0) (size 1.98 3.96) (drill 1.32) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "-") (pintype "passive") (tstamp 93644025-ee30-43f4-a0af-c16131d1cf28))
    (model "${KICAD6_3DMODEL_DIR}/TerminalBlock.3dshapes/TerminalBlock_Altech_AK300-2_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (tstamp e716de49-eda1-409f-a187-cbcb24871b5e)
    (at 96.52 91.44 90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Sheetfile" "led-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "30A Id, 50V Vds, N-Channel Power MOSFET, TO-220")
    (property "ki_keywords" "N-Channel Power MOSFET")
    (path "/15c2dde6-2c28-40a3-b434-60eca1b941fe")
    (attr through_hole)
    (fp_text reference "Q1" (at 2.54 -4.27 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp c90a4207-40b3-4076-827b-4e4235e57c06)
    )
    (fp_text value "BUZ11" (at 2.54 2.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 78565cf9-ca85-4b4b-998c-7375ff86909b)
    )
    (fp_text user "${REFERENCE}" (at 2.54 -4.27 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 399937fe-2ee0-4d51-b04a-e2ba742cc533)
    )
    (fp_line (start -2.58 -3.27) (end -2.58 1.371)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp edf676b0-d91f-4944-8641-2e09cab6b696))
    (fp_line (start -2.58 -3.27) (end 7.66 -3.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 74b225ed-12c6-4dd1-9865-b17697dd8840))
    (fp_line (start -2.58 -1.76) (end 7.66 -1.76)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 84305c56-8ae1-4b83-9f3f-c48c3f93cce0))
    (fp_line (start -2.58 1.371) (end 7.66 1.371)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp cf0852be-e495-4ae2-90ec-6c3620887ada))
    (fp_line (start 0.69 -3.27) (end 0.69 -1.76)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f40d1243-292f-405a-97d5-7b17502bb8ea))
    (fp_line (start 4.391 -3.27) (end 4.391 -1.76)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 60454ba7-a4ea-4ad0-a559-09afaf51e872))
    (fp_line (start 7.66 -3.27) (end 7.66 1.371)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 8f018d1f-8e0b-4af6-aa16-fd4c4567933c))
    (fp_line (start -2.71 -3.4) (end -2.71 1.51)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 10f68fce-aa0a-4dfd-8eb2-b2237f13ddc3))
    (fp_line (start -2.71 1.51) (end 7.79 1.51)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp f202ef6e-82a6-43ec-b194-ccdde113c6ef))
    (fp_line (start 7.79 -3.4) (end -2.71 -3.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 851bd725-20cd-48ac-b172-ff74b7f13fc6))
    (fp_line (start 7.79 1.51) (end 7.79 -3.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 16527919-069a-4c07-9eef-72a9f3c17d0f))
    (fp_line (start -2.46 -3.15) (end -2.46 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 4c3cff54-3b26-484e-bd92-26df64e58549))
    (fp_line (start -2.46 -1.88) (end 7.54 -1.88)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 63d7c449-1f8e-4789-9290-4182a191d80c))
    (fp_line (start -2.46 1.25) (end 7.54 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 9eee873c-2aed-495a-bebf-6c28125825eb))
    (fp_line (start 0.69 -3.15) (end 0.69 -1.88)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp d82b7a16-8025-4727-a67a-9a25961c0eff))
    (fp_line (start 4.39 -3.15) (end 4.39 -1.88)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 1b9fbd7e-67b5-4498-8949-82919c1a8b7a))
    (fp_line (start 7.54 -3.15) (end -2.46 -3.15)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 6f050c6d-434a-4b15-ad08-fbeb5f109f8e))
    (fp_line (start 7.54 1.25) (end 7.54 -3.15)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 156ebfd7-c3ab-4738-9b78-7b5988620a56))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 9 "Net-(J2-Pin_3)") (pinfunction "G") (pintype "input") (tstamp 581e0052-f26c-4471-9737-5444f0b023e7))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 1 "Net-(J1-Pin_2)") (pinfunction "D") (pintype "passive") (tstamp cb793eb9-7188-47c1-bb50-84507639e798))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "S") (pintype "passive") (tstamp f4c97183-b6d7-41bd-8bba-01a4b4ed9927))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (footprint "Package_TO_SOT_THT:TO-220-3_Vertical" (layer "F.Cu")
    (tstamp f727b156-2bca-4dc2-a39f-3cef4443f739)
    (at 76.2 91.44 90)
    (descr "TO-220-3, Vertical, RM 2.54mm, see https://www.vishay.com/docs/66542/to-220-1.pdf")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (property "Sheetfile" "led-controller.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "30A Id, 50V Vds, N-Channel Power MOSFET, TO-220")
    (property "ki_keywords" "N-Channel Power MOSFET")
    (path "/9eef009a-860c-4127-8cf2-cea04ca1ace4")
    (attr through_hole)
    (fp_text reference "Q3" (at 2.54 -4.27 90) (layer "F.SilkS")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 737769b5-a4ce-4b61-9b7a-5c08ed0d7e4d)
    )
    (fp_text value "BUZ11" (at 2.54 2.5 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 8c1199ff-8572-4bcc-ba10-52e06d5ea1c5)
    )
    (fp_text user "${REFERENCE}" (at 2.54 -4.27 90) (layer "F.Fab")
        (effects (font (size 1 1) (thickness 0.15)))
      (tstamp 31161bd7-c570-42fa-a587-4bede8424827)
    )
    (fp_line (start -2.58 -3.27) (end -2.58 1.371)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp b12a40ae-ef7a-4385-beb9-ef4ef3982aba))
    (fp_line (start -2.58 -3.27) (end 7.66 -3.27)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 038f57d0-a7e7-4e3c-aa5d-455b46f301d2))
    (fp_line (start -2.58 -1.76) (end 7.66 -1.76)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f6c90d3d-8a8f-4aa6-b7af-206b65632a07))
    (fp_line (start -2.58 1.371) (end 7.66 1.371)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp a3a1f360-adc0-4f9e-bf4e-247c75f19624))
    (fp_line (start 0.69 -3.27) (end 0.69 -1.76)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 9f28d532-e7c9-4ce1-a574-6a4effcd9406))
    (fp_line (start 4.391 -3.27) (end 4.391 -1.76)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp 738d49e2-a72b-47bf-b0f0-e3c8e61d0c3f))
    (fp_line (start 7.66 -3.27) (end 7.66 1.371)
      (stroke (width 0.12) (type solid)) (layer "F.SilkS") (tstamp f7b37877-82f9-4c51-add0-4497409e3e86))
    (fp_line (start -2.71 -3.4) (end -2.71 1.51)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 7fafa886-d3b9-4a36-8dfc-4639767e68dd))
    (fp_line (start -2.71 1.51) (end 7.79 1.51)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp ad1f1d7d-822d-4f13-83a7-2decef34b8df))
    (fp_line (start 7.79 -3.4) (end -2.71 -3.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 22469c71-6d0a-4356-b95e-442e4a69dbf1))
    (fp_line (start 7.79 1.51) (end 7.79 -3.4)
      (stroke (width 0.05) (type solid)) (layer "F.CrtYd") (tstamp 416a24b2-a664-4ae2-a27a-29d2fb4b2251))
    (fp_line (start -2.46 -3.15) (end -2.46 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp aec992a7-f288-49a3-9407-e01fa8a510f2))
    (fp_line (start -2.46 -1.88) (end 7.54 -1.88)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp dfd41992-3946-4b71-99cb-4abc3ffb7487))
    (fp_line (start -2.46 1.25) (end 7.54 1.25)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp e9f01719-4e6f-44b0-95d5-a4aeb66d125f))
    (fp_line (start 0.69 -3.15) (end 0.69 -1.88)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 2e2d31e9-7f8c-4b9e-b4f5-cc6138dae6fa))
    (fp_line (start 4.39 -3.15) (end 4.39 -1.88)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp a2e53475-1e4d-45ce-8d86-5925f6f01508))
    (fp_line (start 7.54 -3.15) (end -2.46 -3.15)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 271c953a-deb9-4070-bf6d-146cf33102ce))
    (fp_line (start 7.54 1.25) (end 7.54 -3.15)
      (stroke (width 0.1) (type solid)) (layer "F.Fab") (tstamp 8aaa95c8-79e4-48e7-8136-03a12510e9ea))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 4 "Net-(Q3-G)") (pinfunction "G") (pintype "input") (tstamp 08ab7335-fa26-4b0c-9b9d-517a3dde444e))
    (pad "2" thru_hole oval (at 2.54 0 90) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 5 "Net-(J1-Pin_4)") (pinfunction "D") (pintype "passive") (tstamp 68030950-c851-4c61-bb73-34d955f5e586))
    (pad "3" thru_hole oval (at 5.08 0 90) (size 1.905 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 2 "GND") (pinfunction "S") (pintype "passive") (tstamp b33ac481-ed0c-4816-8d0c-6f8a61cd96f6))
    (model "${KICAD6_3DMODEL_DIR}/Package_TO_SOT_THT.3dshapes/TO-220-3_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )

  (gr_rect (start 67.056 81.28) (end 124.968 121.412)
    (stroke (width 0.1) (type default)) (fill none) (layer "Edge.Cuts") (tstamp 2543f2c9-748e-43f4-83ac-fa090cdbebfa))

  (segment (start 91.44 109.22) (end 81.28 109.22) (width 1) (layer "F.Cu") (net 1) (tstamp 5a4165c9-c5e7-4a03-9c6a-dbdf9902bb4f))
  (segment (start 81.28 109.22) (end 81.28 111.76) (width 1) (layer "F.Cu") (net 1) (tstamp 73f291e0-ede2-4a00-a47f-aee8d740f8d4))
  (segment (start 96.52 88.9) (end 91.44 88.9) (width 1) (layer "F.Cu") (net 1) (tstamp eefff450-6b10-4a0e-9d42-7bf0e09863b0))
  (segment (start 91.44 88.9) (end 91.44 109.22) (width 1) (layer "F.Cu") (net 1) (tstamp feda30a3-0092-4167-8c58-d35118a5babd))
  (segment (start 109.22 88.9) (end 109.22 83.82) (width 1) (layer "F.Cu") (net 2) (tstamp 1883a156-4a5d-4036-8576-13e7f61fd787))
  (segment (start 86.36 83.82) (end 78.74 83.82) (width 1) (layer "F.Cu") (net 2) (tstamp 2ab96ac3-7330-4369-9bce-88a298bf1262))
  (segment (start 96.52 83.82) (end 88.9 83.82) (width 1) (layer "F.Cu") (net 2) (tstamp 2ce5197d-da14-40eb-8ca3-f140beeabc92))
  (segment (start 86.36 83.82) (end 86.36 86.36) (width 1) (layer "F.Cu") (net 2) (tstamp 3352279e-66e6-4145-bde0-84ec6c21abf8))
  (segment (start 109.22 88.9) (end 109.22 91.44) (width 1) (layer "F.Cu") (net 2) (tstamp 37fb9c17-ddee-4eba-af0d-6a874ff402d6))
  (segment (start 99.06 104.14) (end 96.52 104.14) (width 1) (layer "F.Cu") (net 2) (tstamp 45e16aa5-bb80-4298-bf27-efa31148ba1d))
  (segment (start 106.68 101.6) (end 106.68 115.57) (width 0.3) (layer "F.Cu") (net 2) (tstamp 46440555-1f6c-42a9-a812-4c5cd21fe8e9))
  (segment (start 106.67 115.58) (end 102.88 115.58) (width 0.3) (layer "F.Cu") (net 2) (tstamp 4c8a164b-0622-42fe-b4d2-012a08ac9f44))
  (segment (start 88.9 83.82) (end 88.9 104.14) (width 1) (layer "F.Cu") (net 2) (tstamp 5015ea3c-b970-47e5-b653-8523e1c2eb4f))
  (segment (start 99.06 83.82) (end 99.06 104.14) (width 1) (layer "F.Cu") (net 2) (tstamp 552ce05d-47ea-44c5-adb8-6ff06187ceb2))
  (segment (start 106.68 93.98) (end 106.68 101.6) (width 1) (layer "F.Cu") (net 2) (tstamp 6888e498-e30f-49f4-af38-6a768cd225b2))
  (segment (start 109.22 83.82) (end 99.06 83.82) (width 1) (layer "F.Cu") (net 2) (tstamp 69867f3f-3145-4581-8498-9df58a8926f9))
  (segment (start 109.22 91.44) (end 106.68 93.98) (width 1) (layer "F.Cu") (net 2) (tstamp 6b8dea7c-cd6b-4d83-9205-39cb7a59ca97))
  (segment (start 99.06 83.82) (end 96.52 83.82) (width 1) (layer "F.Cu") (net 2) (tstamp 73f632a6-ef43-4f41-a650-a02909f4e9cc))
  (segment (start 88.9 104.14) (end 86.36 104.14) (width 1) (layer "F.Cu") (net 2) (tstamp 7cc28dea-04ba-4ea4-85f3-2316c3712247))
  (segment (start 78.74 104.14) (end 76.2 104.14) (width 1) (layer "F.Cu") (net 2) (tstamp 7ebf2020-ce4a-4906-bb24-7df185c795cf))
  (segment (start 99.61 115.58) (end 97.79 113.76) (width 0.3) (layer "F.Cu") (net 2) (tstamp 8aed127d-9fa2-4d8e-b756-36b7f823436a))
  (segment (start 96.52 83.82) (end 96.52 86.36) (width 1) (layer "F.Cu") (net 2) (tstamp 9101bb98-7022-46f8-839f-7fcd4aa639fb))
  (segment (start 106.68 115.57) (end 106.67 115.58) (width 0.3) (layer "F.Cu") (net 2) (tstamp 963952b7-01a5-42d1-9a44-0f40a9d70c22))
  (segment (start 78.74 83.82) (end 76.2 83.82) (width 1) (layer "F.Cu") (net 2) (tstamp aa8b4756-9b69-428f-9c16-d8a99e851a0d))
  (segment (start 88.9 83.82) (end 86.36 83.82) (width 1) (layer "F.Cu") (net 2) (tstamp bdf8eae7-2fca-4ac9-83b4-b2f476f07362))
  (segment (start 78.74 83.82) (end 78.74 104.14) (width 1) (layer "F.Cu") (net 2) (tstamp da492d7e-3f04-4901-85c2-a725a832c770))
  (segment (start 76.2 83.82) (end 76.2 86.36) (width 1) (layer "F.Cu") (net 2) (tstamp dd7a54ed-a747-4c58-91c2-d1a068df4e63))
  (segment (start 102.88 115.58) (end 99.61 115.58) (width 0.3) (layer "F.Cu") (net 2) (tstamp f072a2db-5802-44ea-971e-02131ac74574))
  (segment (start 114.3 113.03) (end 117.475 113.03) (width 0.3) (layer "B.Cu") (net 2) (tstamp 1a510a80-0b65-4120-8c9a-1125c3bbc557))
  (segment (start 102.87 117.475) (end 102.88 117.465) (width 0.3) (layer "B.Cu") (net 2) (tstamp 52d04003-0044-431e-89ce-ae3722854d55))
  (segment (start 102.88 117.465) (end 102.88 115.58) (width 0.3) (layer "B.Cu") (net 2) (tstamp 7b666926-2c58-491e-bd96-096597530710))
  (segment (start 117.475 113.03) (end 117.475 117.475) (width 0.3) (layer "B.Cu") (net 2) (tstamp 9b93f0c2-bfa7-4d6c-975f-af5ba21e6ae4))
  (segment (start 117.475 117.475) (end 102.87 117.475) (width 0.3) (layer "B.Cu") (net 2) (tstamp cd9e0e46-4aa0-4a17-9165-c83664b34d60))
  (segment (start 81.28 106.68) (end 78.74 106.68) (width 1) (layer "F.Cu") (net 3) (tstamp 305771ae-5680-457e-af73-53a0c18c12b1))
  (segment (start 86.36 88.9) (end 81.28 88.9) (width 1) (layer "F.Cu") (net 3) (tstamp 6068bf2e-8c9c-4c5c-8f76-0c3ab52bc69e))
  (segment (start 78.74 106.68) (end 78.74 111.76) (width 1) (layer "F.Cu") (net 3) (tstamp 7f795c50-daec-4ad4-a10e-cb6ead9ba817))
  (segment (start 81.28 88.9) (end 81.28 106.68) (width 1) (layer "F.Cu") (net 3) (tstamp f777b8f0-dae2-4a92-a42d-0820b9f95a85))
  (segment (start 88.9 116.84) (end 100.965 116.84) (width 0.3) (layer "B.Cu") (net 4) (tstamp 243e621c-118f-49ae-809b-76cade9e57a6))
  (segment (start 100.965 113.03) (end 100.975 113.04) (width 0.3) (layer "B.Cu") (net 4) (tstamp 34083812-9892-4beb-9402-121ed98eb337))
  (segment (start 100.975 113.04) (end 102.88 113.04) (width 0.3) (layer "B.Cu") (net 4) (tstamp 71a5ceba-76fb-496c-b5b9-91fbf8ef08ec))
  (segment (start 100.965 116.84) (end 100.965 113.03) (width 0.3) (layer "B.Cu") (net 4) (tstamp 78f08130-c8be-4af7-9dc0-15fc9dc61661))
  (segment (start 76.2 102.235) (end 88.9 102.235) (width 0.3) (layer "B.Cu") (net 4) (tstamp 8120b054-8acf-449f-ab70-ecd916c3a6dd))
  (segment (start 76.2 91.44) (end 76.2 96.52) (width 0.3) (layer "B.Cu") (net 4) (tstamp 8fafd118-fc39-4f4c-8014-c033b65fd2ac))
  (segment (start 76.2 96.52) (end 76.2 102.235) (width 0.3) (layer "B.Cu") (net 4) (tstamp d8b767a8-bfd6-4dd1-beeb-5303639aa1f5))
  (segment (start 88.9 102.235) (end 88.9 116.84) (width 0.3) (layer "B.Cu") (net 4) (tstamp f7e6d226-cd20-4ec7-b91b-19a208787e4f))
  (segment (start 73.66 88.9) (end 73.66 109.22) (width 1) (layer "F.Cu") (net 5) (tstamp 153b7d39-4e70-44fc-9f5c-675385036d2f))
  (segment (start 76.2 88.9) (end 73.66 88.9) (width 1) (layer "F.Cu") (net 5) (tstamp 4506389a-edd1-4106-bdaa-df8d85295df7))
  (segment (start 73.66 109.22) (end 76.2 111.76) (width 1) (layer "F.Cu") (net 5) (tstamp b299877c-05ce-4209-913f-d8952a2d88a8))
  (segment (start 104.22 101.52) (end 104.14 101.6) (width 1) (layer "F.Cu") (net 6) (tstamp 1cd5820d-fefd-4a37-b515-d326a2f1c0ca))
  (segment (start 104.14 101.6) (end 93.98 111.76) (width 1) (layer "F.Cu") (net 6) (tstamp 256f762e-f100-4499-b534-383b04b3229f))
  (segment (start 93.98 111.76) (end 83.82 111.76) (width 1) (layer "F.Cu") (net 6) (tstamp 8b22e73a-c2c1-4302-b091-b13de0f83001))
  (segment (start 104.22 88.9) (end 104.22 101.52) (width 1) (layer "F.Cu") (net 6) (tstamp bf4eb92b-c793-46d8-aaa3-338ea9cb637f))
  (segment (start 109.23 107.96) (end 110.5 107.96) (width 0.3) (layer "F.Cu") (net 8) (tstamp 48305f45-70ed-4c63-bf25-3294789bdcf5))
  (segment (start 109.22 107.95) (end 109.23 107.96) (width 0.3) (layer "F.Cu") (net 8) (tstamp 6d0d4555-9f25-43aa-8440-7ae225661d64))
  (segment (start 109.22 101.6) (end 109.22 107.95) (width 0.3) (layer "F.Cu") (net 8) (tstamp 9fef9cdd-68d6-4b5e-827c-baabd1c9d540))
  (segment (start 109.22 101.6) (end 109.22 103.505) (width 0.3) (layer "B.Cu") (net 8) (tstamp 05e45614-13a7-45d2-9b9c-797b8f99c638))
  (segment (start 98.425 103.505) (end 98.425 109.855) (width 0.3) (layer "B.Cu") (net 8) (tstamp 143dca6c-3449-47e9-a3e5-d902e5b106d8))
  (segment (start 111.75 107.96) (end 111.76 107.95) (width 0.3) (layer "B.Cu") (net 8) (tstamp 188592c2-3b0e-4aad-a487-ecc52dd0abed))
  (segment (start 112.395 115.57) (end 114.3 115.57) (width 0.3) (layer "B.Cu") (net 8) (tstamp 277826b5-3fea-4a3b-a0f5-3e8812c4dcea))
  (segment (start 111.76 107.95) (end 112.395 108.585) (width 0.3) (layer "B.Cu") (net 8) (tstamp 4367422a-c4fd-4cf8-8b11-1091d141d0b4))
  (segment (start 98.425 109.855) (end 97.79 110.49) (width 0.3) (layer "B.Cu") (net 8) (tstamp 67985059-4f37-4236-bbf7-5c801dc3f3c7))
  (segment (start 112.395 108.585) (end 112.395 115.57) (width 0.3) (layer "B.Cu") (net 8) (tstamp 8acb7a84-416a-4263-b277-be8b1e20995e))
  (segment (start 110.5 107.96) (end 111.75 107.96) (width 0.3) (layer "B.Cu") (net 8) (tstamp bf8ccb72-ffa9-4b7a-883e-3895b6fe4ec0))
  (segment (start 97.79 110.49) (end 97.79 111.76) (width 0.3) (layer "B.Cu") (net 8) (tstamp c6ad1e21-3844-492f-92b9-49d053cc44ae))
  (segment (start 109.22 103.505) (end 98.425 103.505) (width 0.3) (layer "B.Cu") (net 8) (tstamp efa408bb-ec24-44b1-9887-ffc28c8e26f4))
  (segment (start 110.5 115.58) (end 110.5 118.1) (width 0.3) (layer "F.Cu") (net 9) (tstamp 11447ca3-cd91-4117-9fde-2472dc5bfd61))
  (segment (start 110.49 118.11) (end 116.84 118.11) (width 0.3) (layer "F.Cu") (net 9) (tstamp 274ced1c-627c-45cf-a101-24d7e0e6b6d2))
  (segment (start 116.84 110.49) (end 114.3 110.49) (width 0.3) (layer "F.Cu") (net 9) (tstamp 2d7d7b1e-d9e9-42bf-99ef-5146a6540e14))
  (segment (start 114.3 111.78) (end 114.3 111.76) (width 0.3) (layer "F.Cu") (net 9) (tstamp 32d178ee-9af7-48cd-8bf7-3687b0bce892))
  (segment (start 116.84 118.11) (end 116.84 110.49) (width 0.3) (layer "F.Cu") (net 9) (tstamp 6f754d3f-9aa5-4c5f-9eb2-89962c0107e4))
  (segment (start 110.5 118.1) (end 110.49 118.11) (width 0.3) (layer "F.Cu") (net 9) (tstamp 9b091de7-b109-482c-aa7a-8b0ca6af3a64))
  (segment (start 120.65 96.52) (end 120.65 110.49) (width 0.3) (layer "B.Cu") (net 9) (tstamp 0c500762-44bf-4873-8189-93e65bdd47d1))
  (segment (start 120.65 110.49) (end 114.3 110.49) (width 0.3) (layer "B.Cu") (net 9) (tstamp 76a27d75-646d-4bf1-998d-51fa98ac5a35))
  (segment (start 96.52 91.44) (end 96.52 96.52) (width 0.3) (layer "B.Cu") (net 9) (tstamp a806cb16-a7e3-479e-b98d-1446ea47cf1f))
  (segment (start 96.52 96.52) (end 120.65 96.52) (width 0.3) (layer "B.Cu") (net 9) (tstamp dab1652d-1c91-433e-b3d0-ad8d80ec4ba6))
  (segment (start 112.395 107.95) (end 114.3 107.95) (width 0.3) (layer "F.Cu") (net 10) (tstamp 0dae0e8e-4fc2-4585-a4f7-2ec5e98bb60c))
  (segment (start 114.3 109.24) (end 114.3 109.22) (width 0.3) (layer "F.Cu") (net 10) (tstamp 731ecf58-ba97-408a-a567-881a760155eb))
  (segment (start 112.385 113.04) (end 112.395 113.03) (width 0.3) (layer "F.Cu") (net 10) (tstamp 92a75ec3-7b7f-4c4c-9205-715c4c13f828))
  (segment (start 110.5 113.04) (end 112.385 113.04) (width 0.3) (layer "F.Cu") (net 10) (tstamp a340adcc-f716-49dd-8d5d-bc5952bc620f))
  (segment (start 112.395 113.03) (end 112.395 107.95) (width 0.3) (layer "F.Cu") (net 10) (tstamp e7487a32-5d26-40c1-8aa9-f62d4fca7ca6))
  (segment (start 118.11 98.425) (end 118.11 107.95) (width 0.3) (layer "B.Cu") (net 10) (tstamp 0bd820dd-5dc3-4e94-a93c-18c7469de96b))
  (segment (start 86.36 91.44) (end 86.36 96.52) (width 0.3) (layer "B.Cu") (net 10) (tstamp 321e1aee-509c-4817-bf10-29c22641471e))
  (segment (start 86.36 96.52) (end 88.265 98.425) (width 0.3) (layer "B.Cu") (net 10) (tstamp 5551f4c6-9468-4ea5-9bc3-98d32a2c85a2))
  (segment (start 118.11 107.95) (end 114.3 107.95) (width 0.3) (layer "B.Cu") (net 10) (tstamp 6621c0c1-07ba-4f43-a469-8371c9dc5b3a))
  (segment (start 88.265 98.425) (end 118.11 98.425) (width 0.3) (layer "B.Cu") (net 10) (tstamp a5f6b382-5c16-42b9-8077-2b122f8736e4))
  (segment (start 114.3 106.7) (end 114.3 106.68) (width 0.3) (layer "F.Cu") (net 11) (tstamp 780c0818-dd08-4374-8043-4518eff7922e))
  (segment (start 110.5 110.5) (end 107.96 110.5) (width 0.3) (layer "B.Cu") (net 11) (tstamp 8b241140-59c8-47cb-9e05-2de09843f9e9))
  (segment (start 107.95 110.49) (end 107.95 106.045) (width 0.3) (layer "B.Cu") (net 11) (tstamp 8cd1248c-98e1-487c-b100-a3dca30ea889))
  (segment (start 108.585 105.41) (end 114.3 105.41) (width 0.3) (layer "B.Cu") (net 11) (tstamp bb0dc919-fd61-45f5-8e32-387c233fd2c9))
  (segment (start 107.95 106.045) (end 108.585 105.41) (width 0.3) (layer "B.Cu") (net 11) (tstamp dcb6e0e1-1dea-4c90-aaaf-a13c9d2331f4))
  (segment (start 107.96 110.5) (end 107.95 110.49) (width 0.3) (layer "B.Cu") (net 11) (tstamp f931b0c2-01a6-46c0-8f2d-0bee36f1d1bb))
  (segment (start 114.3 103.124) (end 112.268 103.124) (width 0.3) (layer "B.Cu") (net 12) (tstamp 18b6ce75-056f-453d-a070-f5373c0043e2))
  (segment (start 103.124 104.648) (end 103.124 107.96) (width 0.3) (layer "B.Cu") (net 12) (tstamp 431dc10b-8641-4c94-8571-4ebbe421c4ac))
  (segment (start 114.3 102.87) (end 114.3 103.124) (width 0.3) (layer "B.Cu") (net 12) (tstamp 4d4e1a72-af97-42b9-a49a-81feafcc106e))
  (segment (start 112.268 104.648) (end 103.124 104.648) (width 0.3) (layer "B.Cu") (net 12) (tstamp 7bfd3457-de47-43cc-b564-bfda64f98d42))
  (segment (start 112.268 103.124) (end 112.268 104.648) (width 0.3) (layer "B.Cu") (net 12) (tstamp 8d9f8588-f3a3-4d3f-920d-12faf2db4a63))
  (segment (start 103.124 107.96) (end 102.88 107.96) (width 0.3) (layer "B.Cu") (net 12) (tstamp c8789565-cb74-415e-939f-f58cfdb12fc3))

)
