(kicad_sch (version 20230121) (generator eeschema)

  (uuid 19234781-cfb7-49fd-a21d-3d4fd6747fa5)

  (paper "A4")

  (lib_symbols
    (symbol "Converter_ACDC:IRM-03-12" (in_bom yes) (on_board yes)
      (property "Reference" "PS" (at 0 6.35 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Value" "IRM-03-12" (at 0 -6.35 0)
        (effects (font (size 1.27 1.27)))
      )
      (property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-03-xx_THT" (at 0 -8.89 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-03/IRM-03-SPEC.PDF" (at 0 -10.16 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_keywords" "Miniature Module-type Power Supply MeanWell" (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_description" "12V, 250mA, 3W, Isolated, AC-DC, IRM03" (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (property "ki_fp_filters" "Converter*ACDC*MeanWell*IRM*03*THT*" (at 0 0 0)
        (effects (font (size 1.27 1.27)) hide)
      )
      (symbol "IRM-03-12_0_1"
        (rectangle (start -7.62 5.08) (end 7.62 -5.08)
          (stroke (width 0.254) (type default))
          (fill (type background))
        )
        (arc (start -5.334 0.635) (mid -4.699 0.2495) (end -4.064 0.635)
          (stroke (width 0) (type default))
          (fill (type none))
        )
        (arc (start -2.794 0.635) (mid -3.429 1.0072) (end -4.064 0.635)
          (stroke (width 0) (type default))
          (fill (type none))
        )
        (polyline
          (pts
            (xy -5.334 -0.635)
            (xy -2.794 -0.635)
          )
          (stroke (width 0) (type default))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 -2.54)
            (xy 0 -3.81)
          )
          (stroke (width 0) (type default))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
          )
          (stroke (width 0) (type default))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0 1.27)
          )
          (stroke (width 0) (type default))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 5.08)
            (xy 0 3.81)
          )
          (stroke (width 0) (type default))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.794 -0.635)
            (xy 5.334 -0.635)
          )
          (stroke (width 0) (type default))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.794 0.635)
            (xy 3.302 0.635)
          )
          (stroke (width 0) (type default))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 3.81 0.635)
            (xy 4.318 0.635)
          )
          (stroke (width 0) (type default))
          (fill (type none))
        )
        (polyline
          (pts
            (xy 4.826 0.635)
            (xy 5.334 0.635)
          )
          (stroke (width 0) (type default))
          (fill (type none))
        )
      )
      (symbol "IRM-03-12_1_1"
        (pin power_in line (at -10.16 2.54 0) (length 2.54)
          (name "AC/L" (effects (font (size 1.27 1.27))))
          (number "1" (effects (font (size 1.27 1.27))))
        )
        (pin power_out line (at 10.16 -2.54 180) (length 2.54)
          (name "-Vo" (effects (font (size 1.27 1.27))))
          (number "14" (effects (font (size 1.27 1.27))))
        )
        (pin power_out line (at 10.16 2.54 180) (length 2.54)
          (name "+Vo" (effects (font (size 1.27 1.27))))
          (number "16" (effects (font (size 1.27 1.27))))
        )
        (pin power_in line (at -10.16 -2.54 0) (length 2.54)
          (name "AC/N" (effects (font (size 1.27 1.27))))
          (number "3" (effects (font (size 1.27 1.27))))
        )
        (pin no_connect line (at -7.62 0 0) (length 2.54) hide
          (name "NC" (effects (font (size 1.27 1.27))))
          (number "5" (effects (font (size 1.27 1.27))))
        )
      )
    )
  )


  (symbol (lib_id "Converter_ACDC:IRM-03-12") (at 109.22 88.9 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (uuid 3645a35f-038d-4e94-a5da-8babbe5ed916)
    (property "Reference" "PS1" (at 109.22 78.74 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Value" "IRM-03-12" (at 109.22 81.28 0)
      (effects (font (size 1.27 1.27)))
    )
    (property "Footprint" "Converter_ACDC:Converter_ACDC_MeanWell_IRM-03-xx_THT" (at 109.22 97.79 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (property "Datasheet" "https://www.meanwell.com/Upload/PDF/IRM-03/IRM-03-SPEC.PDF" (at 109.22 99.06 0)
      (effects (font (size 1.27 1.27)) hide)
    )
    (pin "1" (uuid 4d66a45e-3bb1-4015-90ad-7c31065555f7))
    (pin "14" (uuid 9c3bb577-aa87-445c-9654-e61772d56db1))
    (pin "16" (uuid a9328313-b151-42ad-aea6-a19a9ac6d32f))
    (pin "3" (uuid 36d4f5e2-bf2d-4124-809d-25643fbb5d42))
    (pin "5" (uuid 2353bcb8-71f0-4240-9d1b-7439e3b8ce13))
    (instances
      (project "pso"
        (path "/19234781-cfb7-49fd-a21d-3d4fd6747fa5"
          (reference "PS1") (unit 1)
        )
      )
    )
  )

  (sheet_instances
    (path "/" (page "1"))
  )
)
